# Coder Assumptions for 'Abstandsensor'

List of assumptions that you can check and expected results for selected target environment. For more information see, Verification of Code Generation Assumptions.

### C Language Configuration for Atmel->AVR Target Hardware

BitPerChar | 8
BitPerShort | 16
BitPerInt | 16
BitPerLong | 32
BitPerFloat | 32
BitPerDouble | 64
BitPerPointer | 16
BitPerSizeT | 16
BitPerPtrDiffT | 16
Endianness | LittleEndian
Shift right for signed integer is arithmetic shift. | True
Signed integer division rounds to | Zero

### Floating-Point Numbers

Code generation is configured to support floating-point numbers. Target environment might perform subnormal number calculations.
Flush-to-zero computed subnormal values (FTZ). | False
Flush-to-zero incoming subnormal values (DAZ). | False
If assumptions are not correct, subnormal numbers might cause mismatches between model and generated code simulation results. For more information see, Subnormal Number Performance.